Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1184	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	05/06/92	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7796072 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	382060  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Dy3.52
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Aristida species, Digitaria 
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Petalostigma 
	pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subrounded, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/3-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric;
	 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Clear change to - 
	B21	0.1 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy fabric; 2-
	10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, ,
	 ; Gradual change to - 
	B22	0.6 - 0.9 m	Light olive brown (2.5Y5/4-Moist); Mottles, 7.5YR54, 10-20% , Distinct; Mottles, 10-20% ; Sandy 
	light medium clay; Massive grade of structure; Earthy fabric; 20-50%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1184	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.3A
	0.1 - 0.6	6.2A
	0.6 - 0.9	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.6
	0.6 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.6
	0.6 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1184	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension