Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1202	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	17/06/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7850768 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	381866  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Medium Very gravelly 	Principal Profile Form:	Dy3.12
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa species, Aristida species
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, rounded, Quartz
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (7.5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; 20-50%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	A12	0.08 - 0.2 m	Dark brown (7.5YR3/4-Moist); ; Clay loam, sandy; Massive grade of structure; Sandy (grains 
	prominent) fabric; 20-50%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.15); Abrupt change to - 
	B21	0.2 - 0.55 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; , 
	Lenticular; Smooth-ped fabric; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Common cutans, 10-50% of ped faces or walls coated; , Calcareous, , ; , Gypseous, 
	, ; Field pH 8.5 (Raupach, 0.3); Gradual change to - 
	B22	0.55 - 1 m	Strong brown (7.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; 
	Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); Gradual change 
	to - 
	B23	1 - 1.2 m	Strong brown (7.5YR4/6-Moist); Mottles, 5Y62, 10-20% , Distinct; Mottles, 10-20% ; Medium clay;
	 Weak grade of structure, Angular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1202	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1202	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile