Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	121	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	24/08/90	Elevation:	415 metres
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7848621 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	319061  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous-Endohypersodic Self-Mulching Black 	Principal Profile Form:	Ug5.15
	Vertosol Non-gravelly Medium fine Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Paspalum species, Enteropogon species, 
	Bothriochloa bladhii	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Strong grade of structure, <2 mm,
	 Granular; Smooth-ped fabric; Medium, (5 - 10) mm crack; Moderately moist; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9.9 (Raupach, 0.05); Many, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B21	0.08 - 1.5 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 
	mm, Lenticular; Smooth-ped fabric; Moist; Firm consistence; Many cutans, >50% of ped faces 
	or walls coated, prominent; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Concretions; , 
	Gypseous, , ; Field pH 9.9 (Raupach, 0.9); Few, very fine (0-1mm) roots; Clear, Smooth change 
	to - 
	B22k	1.5 - 2 m	Dark brown (10YR3/3-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Lenticular; 
	Moderately moist; Firm consistence; Many cutans, >50% of ped faces or walls coated, 
	prominent; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Nodules; , Gypseous, , ; Field
	 pH 9.9 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	121	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.8A	37B	31	0.54	1.3	71B	1.83
	33E	31	0.59	1.4	1.97
	0.08 - 1.5	8.9A	22B	37	0.66	9.7	67B	14.48
	20E	34	0.71	8.9	49.6I	19.56
	14J	20.2	0.4	6.8	13.28
	17.94
	10.15
	13.71
	1.5 - 2	9.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 1.5
	1.5 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 1.5
	1.5 - 2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	121	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension