Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	19/06/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7837930 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	388917  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Supracalcic Subnatric Brown Sodosol Medium Non-gravelly 	Principal Profile Form:	Db1.23
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - Aristida species, Chrysopogon fallax, Chloris 
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, subrounded, Quartz
	Profile Morphology
	A11	0 - 0.08 m	Brown (7.5YR4/2-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.03); Clear change to - 
	A2	0.08 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; 20-50%,
	 cobbly, 60-200mm, subangular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field
	 pH 6.5 (Raupach, 0.15); Abrupt change to - 
	B21	0.2 - 0.55 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.3); 
	Clear change to - 
	B22	0.55 - 0.7 m	Yellowish brown (10YR5/4-Moist); ; Sandy medium heavy clay; Weak grade of structure, 5-10 
	mm, Polyhedral; Smooth-ped fabric; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft 
	segregations; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.3A	0.86B	0.65	0.21	0.04
	0.08 - 0.2	7A
	0.2 - 0.55	7.6A
	0.55 - 0.7	8.7A	9.1B	12	0.11	3.6
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.2
	0.2 - 0.55
	0.55 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.2
	0.2 - 0.55
	0.55 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension