Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1227	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	30/06/92	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7861814 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	392678  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Dermosol Medium Non-gravelly 	Principal Profile Form:	Uf6.31
	Clayey Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Dichanthium species, 
	Bothriochloa species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Dark reddish brown (5YR3/2-Moist); ; Fine sandy light clay; Massive grade of structure; Earthy 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Clear change to - 
	A12	0.08 - 0.22 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.15); Gradual change to - 
	B21	0.22 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.4); Clear change to - 
	B22	0.6 - 1 m	Yellowish red (5YR4/6-Moist); ; Light medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly 
	calcareous; Field pH 8 (Raupach, 0.8); Clear change to - 
	B23	1 - 1.2 m	Yellowish red (5YR4/6-Moist); Mottles, 7.5YR44, 20-50% , Prominent; Mottles, 20-50% ; Light 
	medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Few (2
	 - 10 %), Manganiferous, , Soft segregations; Common (10 - 20 %), Calcareous, Medium (2 -6 
	mm), Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1227	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1227	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile