Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1233	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	30/06/92	Elevation:	380 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7864079 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	386602  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Low hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Medium Non-gravelly Loamy 	Principal Profile Form:	Gn2.11
	Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Aristida species, Cyperus 
	species	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Planchonia careya, Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa, Eucalyptus papuana
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 2-10%, 
	fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.25 m	Dark reddish brown (5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Many (20 - 50 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous,
	 , ; Field pH 6 (Raupach, 0.15); Clear change to - 
	B22	0.25 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 2-
	10%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1233	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A
	0.1 - 0.25	6.5A
	0.25 - 0.5	6.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1233	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension