Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1238	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	01/06/92	Elevation:	360 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7853931 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	367175  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Brown Sodosol Medium Gravelly Loamy 	Principal Profile Form:	Dy2.43
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Aristida species, Cynodon 
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus persistens
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus persistens
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, angular, Granite
	Profile Morphology
	A	0 - 0.02 m	Brown (10YR4/3-Moist); ; Sandy loam; Weak grade of structure, Platy; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.01); Abrupt change to - 
	A2e	0.02 - 0.17 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Abrupt change to - 
	B21	0.17 - 0.3 m	Dark greyish brown (2.5Y4/3-Moist); ; Medium clay (Light); Moderate grade of structure, 
	Subangular blocky; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.25); Clear change to 
	- 
	B22	0.3 - 0.5 m	Light olive brown (2.5Y5/4-Moist); ; Medium clay; Moderate grade of structure, Subangular 
	blocky; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1238	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	5.9A
	0.02 - 0.17	6.5A
	0.17 - 0.3	7.7A
	0.3 - 0.5	8.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.17
	0.17 - 0.3
	0.3 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.17
	0.17 - 0.3
	0.3 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1238	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension