Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	03/09/90	Elevation:	410 metres
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7782192 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	351559  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	130 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Eutrophic Brown Ferrosol Medium Non-gravelly 	Principal Profile Form:	Gn3.72
	Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa ewartiana, Aristida species, 
	Heteropogon contortus	Mid Strata - Tree, 1.01-3m, Isolated clumps. *Species includes - Eucalyptus papuana, Bursaria incana
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus papuana, Eucalyptus crebra, Bursaria incana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/3-Moist); ; Clay loam (Heavy); Moderate grade of structure, 5-10 mm, 
	Polyhedral; Smooth-ped fabric; Moderately moist; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0); Common, very fine (0-1mm) roots; Clear, Smooth 
	change to - 
	B1	0.1 - 0.53 m	Reddish brown (5YR4/4-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; 
	Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 
	0.3); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B2c	0.53 - 1.6 m	Strong brown (7.5YR5/8-Moist); Mottles, 7.5YR68, 10-20% , 0-5mm, Distinct; Mottles, 10-20% ; 
	Light clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Moderately moist; Weak consistence; Very many (50 - 100 %), Ferromanganiferous, Coarse (6 - 
	20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 1.2); Few, very fine (0-
	1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.2A	9.7B	2.9	1.2	0.06
	0.1 - 0.53	7A
	0.53 - 1.6	7A	5.8B	3.6	0.43	0.08	11I	0.73
	5.5J	2.2	0.6	0.1	0.91
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.53
	0.53 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.53
	0.53 - 1.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	124	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension