Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1258	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	29/06/92	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7856280 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	392596  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroferric Yellow Kandosol Medium Non-gravelly 	Principal Profile Form:	Dy3.62
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Themeda triandra, 
	Phynchelytrum repens	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Melaleuca nervosa, Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.11 m	Very dark grey (10YR3/1-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	A12	0.11 - 0.23 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Weak 
	consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, 
	, ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); Clear change to - 
	B21	0.23 - 0.55 m	Dark yellowish brown (10YR3/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy 
	fabric; Weak consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; ,
	 Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear change to - 
	B22	0.55 - 0.65 m	Olive yellow (2.5Y6/6-Moist); Mottles, 5YR58, 2-10% , Distinct; Mottles, 2-10% ; Sandy light clay;
	 Massive grade of structure; Sandy (grains prominent) fabric; Firm consistence; 2-10%, fine 
	gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1258	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	7.2A	1.5B	0.84	0.23	0.06
	0.23 - 0.55	6.7A	1.2B	1.1	0.18	0.04
	0.55 - 0.65	6.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.23 - 0.55
	0.55 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.23 - 0.55
	0.55 - 0.65

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1258	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension