Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1260	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	29/06/92	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7858582 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	392550  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Self-mulching, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Self-Mulching Black Vertosol Slightly 	Principal Profile Form:	Ug5.16
	gravelly Medium fine Medium fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Cynodon dactylon
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subrounded, Quartz
	Profile Morphology
	A11	0 - 0.17 m	Black (7.5YR2/0-Moist); ; Light medium clay; Strong grade of structure, Polyhedral; Smooth-ped 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	B21	0.17 - 0.4 m	Black (7.5YR2/0-Moist); ; Medium clay; Moderate grade of structure, Subangular blocky; Smooth-
	ped fabric; , Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly calcareous; Field pH 8 
	(Raupach, 0.25); Clear change to - 
	B22	0.4 - 0.75 m	Black (7.5YR2/0-Moist); ; Medium clay; Moderate grade of structure, Lenticular; Smooth-ped 
	fabric; Common (10 - 20 %), Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; Soil matrix
	 is Highly calcareous; Field pH 9 (Raupach, 0.6); Abrupt change to - 
	C	0.75 - 1.4 m	Reddish brown (5YR5/3-Moist); ; Clay loam; Moderate grade of structure, Platy; Smooth-ped 
	fabric; Many (20 - 50 %), Calcareous, , Soft segregations; , Gypseous, , ; Soil matrix is Highly 
	calcareous; Field pH 9 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1260	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1260	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile