Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/07/92	Elevation:	460 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7864362 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	353375  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Terrace flat	Slope Category:	Level
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Paralithic Orthic Tenosol Thin Non-gravelly Loamy 	Principal Profile Form:	Uc5.11
	Loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Heteropogon contortus, Chrysopogon fallax, Elionurus citreus
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent)
	 fabric; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	B1	0.08 - 0.3 m	Brown (7.5YR4/4-Moist); ; Clayey fine sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); Clear change to - 
	B21	0.3 - 0.7 m	Brown (7.5YR5/4-Moist); ; Clayey fine sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Clear change to - 
	B22	0.7 - 0.95 m	Light yellowish brown (10YR6/4-Moist); ; Fine sandy loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6A	2.7B	0.86	0.38	0.03
	0.08 - 0.3	6.1A
	0.3 - 0.7	6.4A	1.3B	0.55	0.23	0.03
	0.7 - 0.95	6.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.7
	0.7 - 0.95
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.7
	0.7 - 0.95

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension