Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1284	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	22/07/92	Elevation:	400 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7871174 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	351312  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Um5.52
	loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Bothriochloa pertusa, Themeda triandra, 
	Bothriochloa decipiens	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus persistens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus persistens
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.13 m	Dark yellowish brown (10YR4/4-Moist); ; Fine sandy clay loam; Massive grade of structure; Weak
	 grade of structure; Sandy (grains prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6.5
	 (Raupach, 0.03); Abrupt change to - 
	A12	0.13 - 0.25 m	Dark brown (10YR3/3-Moist); ; Clay loam, fine sandy; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.2); Clear change to - 
	B2	0.25 - 0.45 m	Brown (10YR4/3-Moist); ; Clay loam, fine sandy; Weak grade of structure, 20-50 mm, Subangular
	 blocky; , Platy; Rough-ped fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1284	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6A
	0.13 - 0.25	5.9A
	0.25 - 0.45	6.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13
	0.13 - 0.25
	0.25 - 0.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.25
	0.25 - 0.45

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1284	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension