Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1290	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/07/92	Elevation:	308 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7856684 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	357965  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Paralithic Orthic Tenosol Medium Non-gravelly Sandy 	Principal Profile Form:	Uc5.21
	Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Heteropogon contortus, Digitaria
	 species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent)
	 fabric; 2-10%, fine gravelly, 2-6mm, angular, Granite, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.02); Abrupt change to - 
	A12	0.03 - 0.17 m	Dark brown (7.5YR3/4-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; 10-20%, fine gravelly, 2-6mm, angular, Granite, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear change to - 
	B21	0.17 - 0.28 m	Strong brown (7.5YR4/6-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; 20-50%, fine gravelly, 2-6mm, angular, Granite, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B3	0.28 - 0.45 m	Strong brown (7.5YR5/6-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; 50-90%,
	 fine gravelly, 2-6mm, angular, Granite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7 (Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1290	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1290	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile