Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1291	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/07/92	Elevation:	380 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7856924 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	360388  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Kandosol Medium Non-gravelly 	Principal Profile Form:	Um5.52
	Clay-loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa decipiens
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus polycarpa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy clay loam; Massive grade of structure; 
	Earthy fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Abrupt change to - 
	A12	0.05 - 0.27 m	Dark brown (7.5YR3/3-Moist); ; Fine sandy clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B21	0.27 - 0.7 m	Brown (7.5YR4/4-Moist); ; Fine sandy clay loam (Light); Massive grade of structure; Earthy fabric;
	 20-50%, fine gravelly, 2-6mm, angular, Granite, coarse fragments; , Calcareous, , ; , Gypseous, 
	, ; Field pH 6 (Raupach, 0.5); Clear change to - 
	B22	0.7 - 0.95 m	Strong brown (7.5YR4/6-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric;
	 , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1291	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A	7.7B	1.9	0.87	0.08
	0.05 - 0.27	6.1A
	0.27 - 0.7	6A	3B	0.71	0.27	0.04
	0.7 - 0.95	6.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.27
	0.27 - 0.7
	0.7 - 0.95
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.27
	0.27 - 0.7
	0.7 - 0.95

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1291	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension