Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1300	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	24/07/92	Elevation:	360 metres
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7863079 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	384245  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Metamorphic rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	Dy3.11
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Dichanthium species, 
	Heteropogon contortus	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Atalaya hemiglauca
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus persistens, Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, angular, 
	Profile Morphology
	A11	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Clear change to - 
	A12	0.05 - 0.12 m	Brown (10YR4/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; 10-
	20%, medium gravelly, 6-20mm, angular, Metamorphic rock (unidentified), coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Abrupt change to - 
	B21	0.12 - 0.4 m	Yellowish brown (10YR5/4-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Polyhedral; Smooth-ped fabric; 10-20%, medium gravelly, 6-20mm, angular, Metamorphic rock 
	(unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Clear change to - 
	B22	0.4 - 0.55 m	Dark greyish brown (2.5Y4/3-Moist); Mottles, 5YR44, 10-20% , Faint; Mottles, 10-20% ; Medium 
	clay; Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-ped fabric; 20-50%, coarse 
	gravelly, 20-60mm, angular, Metamorphic rock (unidentified), coarse fragments; , Calcareous, , ; 
	, Gypseous, , ; Field pH 6 (Raupach, 0.5); Clear change to - 
	C	0.55 - 0.6 m	; 50-90%, coarse gravelly, 20-60mm, angular, Metamorphic rock (unidentified), coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1300	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2A
	0.05 - 0.12	6.1A
	0.12 - 0.4	6.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.12
	0.12 - 0.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.12
	0.12 - 0.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1300	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension