Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	04/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7894792 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	373341  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Thick Non-gravelly Clay-	Principal Profile Form:	Gn2.11
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Themeda triandra, Panicum species, Chrysopogon 
	fallax	Mid Strata - Tree, 1.01-3m, Mid-dense. *Species includes - Acacia species, Eucalyptus similis
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus similis, Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.15 m	Dark reddish brown (5YR3/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.1); Clear 
	change to - 
	A12	0.15 - 0.3 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric;
	 Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); Gradual 
	change to - 
	B2	0.3 - 0.8 m	Dark red (2.5YR3/6-Moist); Mottles, 7.5YR56, 0-2% , 5-15mm, Distinct; Mottles, 0-2% ; Sandy 
	light clay; Massive grade of structure; Weak grade of structure, 10-20 mm, Polyhedral; Earthy 
	fabric; Moderately moist; Very firm consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.7A
	0.15 - 0.3	5.8A
	0.3 - 0.8	5.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension