Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1323	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	05/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7886946 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	367082  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Low hills
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	10 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol Medium Very gravelly Clay-	Principal Profile Form:	Dr3.12
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Themeda triandra, Dichanthium species, Heteropogon
	 contortus	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana, Grevillea parallela
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	50-90%, cobbly, 60-200mm, subangular, 
	Profile Morphology
	A11	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; 20-50%, fine gravelly, 2-6mm, angular, Granite, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt change to - 
	A12	0.1 - 0.16 m	Dark yellowish brown (10YR4/4-Moist); ; Clay loam, sandy (Heavy); Massive grade of structure; 
	Earthy fabric; 2-10%, medium gravelly, 6-20mm, angular, Granite, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Abrupt change to - 
	B21	0.16 - 0.45 m	Yellowish red (5YR4/6-Moist); Mottles, 10-20% , Faint; Mottles, 10-20% ; Medium heavy clay; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.3); Clear change to - 
	B22	0.45 - 0.6 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Soft 
	segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.5); Gradual change to - 
	B3	0.6 - 1.3 m	Dark yellowish brown (10YR4/6-Moist); Mottles, 2-10% , Distinct; Mottles, 2-10% ; Clay loam; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Few (2 - 10 %), 
	Manganiferous, Fine (0 - 2 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1323	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.8A
	0.16 - 0.45	7.1A
	0.6 - 1.3	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.16 - 0.45
	0.6 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.16 - 0.45
	0.6 - 1.3

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1323	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension