Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1331	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	06/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7897608 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	361656  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Chromosol Thick Non-gravelly 	Principal Profile Form:	Db3.12
	Sandy Clayey Deep
	ASC Confidence:	Great Soil Group:	Brown podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Bothriochloa decipiens, 
	Phynchelytrum repens	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.09 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.05); Clear change to - 
	A12	0.09 - 0.3 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); Clear change to - 
	B2	0.3 - 0.7 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Clear change to - 
	D	0.7 - 1.3 m	Dark brown (7.5YR3/4-Moist); ; Sandy light clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Few (2 - 10 %), Manganiferous, , Soft segregations; ,
	 Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1331	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	6.5A
	0.09 - 0.3	6.8A
	0.3 - 0.7	6.9A
	0.7 - 1.3	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09
	0.09 - 0.3
	0.3 - 0.7
	0.7 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.3
	0.3 - 0.7
	0.7 - 1.3

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1331	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension