Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1332	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	06/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7895064 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	358982  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Grey Chromosol Medium Slightly gravelly 	Principal Profile Form:	Dy3.12
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa decipiens, Chrysopogon fallax
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, 
	Profile Morphology
	A11	0 - 0.12 m	Dark brown (10YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 10-
	20%, medium gravelly, 6-20mm, subrounded, Substrate material, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A12	0.12 - 0.27 m	Brown (10YR4/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 20-50%, 
	subrounded, Substrate material, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.2); Abrupt change to - 
	B21	0.27 - 0.45 m	Dark greyish brown (10YR4/2-Moist); Mottles, 2.5YR46, 2-10% , Distinct; Mottles, 2-10% ; 
	Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-ped fabric; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Very few (0 - 2 %), Manganiferous, Fine (0 - 2 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.35); Clear change to - 
	B22	0.45 - 0.6 m	Dark greyish brown (10YR4/2-Moist); Mottles, 10YR56, 2-10% , Distinct; Mottles, 2-10% ; Medium
	 clay; Moderate grade of structure, 10-20 mm, Polyhedral; Smooth-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.5); 
	C	0.6 - 0.8 m	; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1332	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.1A
	0.12 - 0.22	6.6A
	0.22 - 0.45	7.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.22
	0.22 - 0.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.22
	0.22 - 0.45

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1332	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension