Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	07/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7880832 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	386257  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Paralithic Orthic Tenosol Medium Non-gravelly Sandy 	Principal Profile Form:	Uc5.11
	Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - Aristida species
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Grevillea glauca, Melaleuca nervosa, Petalostigma 
	pubescens
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.06 m	Dark brown (7.5YR3/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear change to -
	A12	0.06 - 0.22 m	Strong brown (7.5YR4/6-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Clear change 
	to - 
	B/A	0.22 - 0.5 m	Yellowish red (5YR5/8-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.8A	1.7B	0.45	0.23	0.03
	0.22 - 0.5	6.5A	0.81B	0.51	0.22	0.04
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.22 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.22 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension