Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1348	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	12/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7780356 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	332192  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol Thin Moderately gravelly 	Principal Profile Form:	Uf6.31
	Clayey Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa species
	Mid Strata - , , . *Species includes - Eucalyptus polycarpa, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus platyphylla, Eucalyptus 
	Surface Coarse Fragments:	20-50%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); ; Light clay; Moderate grade of structure, Polyhedral; Smooth-ped 
	fabric; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.03); Clear change to - 
	B21	0.05 - 0.3 m	Brown (7.5YR4/4-Moist); ; Light clay; Massive grade of structure; Weak grade of structure; Earthy
	 fabric; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B22	0.3 - 0.7 m	Strong brown (7.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Common 
	(10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.5); Gradual change to - 
	B23	0.7 - 0.8 m	Strong brown (7.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Common 
	(10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1348	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.6A
	0.05 - 0.3	6.3A
	0.7 - 0.8	6.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.3
	0.7 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.3
	0.7 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1348	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension