Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	19/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7750860 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	319738  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Dermosol Thin Gravelly Clay-loamy 	Principal Profile Form:	Gn3.52
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Aristida species, Panicum species, Heteropogon 
	contortus	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus similis, Acacia species, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus similis, Eucalyptus papuana
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, angular, Granite
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (7.5YR3/3-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; Dry; 
	2-10%, fine gravelly, 2-6mm, subangular, Granite, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Abrupt change to - 
	B1	0.05 - 0.25 m	Reddish brown (5YR4/4-Moist); ; Sandy light clay; Massive grade of structure; Earthy fabric; Dry; 
	2-10%, fine gravelly, 2-6mm, subangular, Granite, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Clear change to - 
	B21	0.25 - 0.45 m	Yellowish red (5YR4/6-Moist); Mottles, 10YR56, 10-20% , Faint; Mottles, 10-20% ; Light medium 
	clay; Moderate grade of structure, 20-50 mm, Polyhedral; Smooth-ped fabric; Dry; 10-20%, 
	medium gravelly, 6-20mm, subrounded, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7 (Raupach, 0.4); Gradual change to - 
	B22	0.45 - 0.8 m	Light olive brown (2.5Y5/4-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, 
	Lenticular; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; 
	Moderately moist; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2
	 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	(Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.4A	6.6B	3	0.44	0.08
	0.05 - 0.25	6.1A
	0.45 - 0.8	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.25
	0.45 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.25
	0.45 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension