Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1383	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7777002 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	313567  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Ferrosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.22
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Dichanthium species, Themeda triandra, Heteropogon
	 contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, 
	Granular; Smooth-ped fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6
	 (Raupach, 0.05); Abrupt change to - 
	A12	0.05 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.1); Clear change to - 
	B21	0.1 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.25); Clear change to - 
	B22	0.3 - 0.65 m	Yellow (10YR8/6-Moist); Mottles, 7.5YR46, 0-2% , 0-5mm, Faint; Mottles, 0-2% ; Light clay; 
	Strong grade of structure, 5-10 mm, Polyhedral; Smooth-ped fabric; Dry; Firm consistence; Few 
	(2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.6); Gradual change to - 
	B23	0.65 - 1 m	Reddish yellow (7.5YR8/6-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Firm consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); Clear change to - 
	C	1 - 1.1 m	; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1383	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A
	0.1 - 0.3	6.4A
	0.65 - 1	7.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.1 - 0.3
	0.65 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.1 - 0.3
	0.65 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1383	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension