Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1384	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	21/08/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7786684 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	299168  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thin Non-gravelly Clayey 	Principal Profile Form:	Uf6.21
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Themeda triandra, Heteropogon contortus, 
	Bothriochloa species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus orgadophylla, Eucalyptus crebra, Brachychiton 
	populneus
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, subangular, Basalt
	Profile Morphology
	A1	0 - 0.06 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear 
	change to - 
	B21	0.06 - 0.4 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Gradual change to -
	B22	0.4 - 0.8 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric;  Very fine (0.075-1mm) macropores, Dry; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1384	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.8A
	0.06 - 0.4	6.9A
	0.4 - 0.8	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.06 - 0.4
	0.4 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.4
	0.4 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1384	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension