Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1392	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	14/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7781151 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	388634  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroferric Red Kandosol Medium Clay-loamy Clayey 	Principal Profile Form:	Gn2.22
	Shallow 
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Aristida species, Sporobolus caroli
	Mid Strata - Tree, 6.01-12m, Very sparse. *Species includes - Acacia salicina, Bursaria incana
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.05); Abrupt change 
	to - 
	A12	0.1 - 0.25 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric;
	 Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear 
	change to - 
	B2	0.25 - 0.4 m	Light red (2.5YR6/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.35); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1392	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1392	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile