Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1406	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	15/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7733347 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	360062  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Petroferric Brown Kandosol     	Principal Profile Form:	Gn2.62
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.51-1m, Mid-dense. *Species includes - Triodia mitchelii, Aristida species, Eriachne 
	Mid Strata - Tree, 6.01-12m, Very sparse. *Species includes - Bursaria incana, Eucalyptus melanophloia
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus polycarpa, Eucalyptus 
	papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.28 m	Yellowish brown (10YR5/6-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Clear change to - 
	B21	0.28 - 0.75 m	Light olive brown (2.5Y5/6-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.5); Gradual change to - 
	B22	0.75 - 1.05 m	Light olive brown (2.5Y5/6-Moist); Mottles, 2.5Y46, 10-20% , Distinct; Mottles, 10-20% ; Sandy 
	light clay; Massive grade of structure; Earthy fabric; Dry; 10-20%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1406	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	1.9B	1.1	0.4	0.06
	0.1 - 0.28	5.6A
	0.28 - 0.75	5.7A	1.3B	1.9	0.22	0.22
	0.75 - 1.05	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.28
	0.28 - 0.75
	0.75 - 1.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.28
	0.28 - 0.75
	0.75 - 1.05

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1406	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension