Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1410	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	16/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7748920 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	392057  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol     	Principal Profile Form:	Gn3.12
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species, Bothriochloa species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus shirleyi
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, , subrounded, Ferricrete
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (7.5YR3/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt 
	change to - 
	B1	0.08 - 0.25 m	Strong brown (7.5YR4/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; 10-20%, medium gravelly, 6-20mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B21	0.25 - 0.5 m	Strong brown (7.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Weak consistence; Many (20 - 50 %), Ferromanganiferous, Medium (2 -6
	 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.45); Clear change to - 
	B22	0.5 - 0.8 m	Red (2.5YR4/6-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Polyhedral; Smooth-ped 
	fabric; Dry; Very firm consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1410	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.6A
	0.25 - 0.5	6.5A
	0.5 - 0.8	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.25 - 0.5
	0.5 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.25 - 0.5
	0.5 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1410	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension