Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1419	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	17/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7747702 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	353243  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mellic Brown Kandosol     	Principal Profile Form:	Um5.41
	ASC Confidence:	Great Soil Group:	Lithosol
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - Cyperus species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus platyphylla, Eucalyptus crebra
	Surface Coarse Fragments:	90-100%, coarse gravelly, 20-60mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; 50-90%, coarse gravelly, 20-60mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.05); Gradual change to - 
	BC	0.1 - 0.25 m	Dark yellowish brown (10YR4/4-Moist); ; Clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; 50-90%, coarse gravelly, 20-60mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1419	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.6A
	0.1 - 0.25	5.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1419	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension