Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1475	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	13/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7731407 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	359693  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Bleached-Leptic Tenosol Thick Non-	Principal Profile Form:	Uc2
	gravelly Sandy Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species, Heteropogon contortus
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Petalostigma pubescens, Acacia species
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus polycarpa, Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.18 m	Brown (10YR4/3-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Gradual change to - 
	A12	0.18 - 0.35 m	Yellowish brown (10YR5/4-Moist); ; Loamy sand; Single grain grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Gradual change to - 
	A2e	0.35 - 0.55 m	Yellowish brown (10YR5/6-Moist); ; Loamy sand; Single grain grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1475	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1475	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile