Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	07/09/90	Elevation:	395 metres
	Map Ref.:	Sheet No. : 8060   GPS	Rainfall:	No Data
	Northing/Long.:	7906028 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	361205  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Thick Non-	Principal Profile Form:	Dy3.33
	gravelly Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Dichanthium sericeum, Heteropogon contortus, 
	Urochloa mosambicensis	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, angular, 
	Profile Morphology
	A1	0 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy clay loam (Light); Massive grade of structure; 
	Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; 20-
	50%, fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.05); Abundant, fine (1-2mm) roots; Clear, Smooth change 
	to - 
	A2j	0.15 - 0.3 m	Brown (10YR4/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; 50-90%, medium gravelly, 
	6-20mm, subrounded, dispersed, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.5 (Raupach, 0.3); Many, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B21c	0.3 - 0.95 m	Yellowish brown (10YR5/8-Moist); Mottles, 5YR58, 20-50% , 0-5mm, Distinct; Mottles, 20-50% ; 
	Medium clay; Strong grade of structure, 20-50 mm, Prismatic; Strong grade of structure, 10-20 
	mm, Angular blocky; Smooth-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Very firm consistence; Common cutans, 10-50% of ped faces or walls 
	coated, prominent; Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, 
	, ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Many, fine (1-2mm) roots; Clear, Smooth change to 
	B22	0.95 - 1.3 m	Yellowish brown (10YR5/6-Moist); Mottles, 10YR42, 20-50% , 5-15mm, Prominent; Mottles, 20-
	50% ; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Many (>5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Very firm consistence; Common cutans, 
	10-50% of ped faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 1.2); Common, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.3A	2.4B	1.5	0.39	0.05
	0.15 - 0.3	6.7A
	0.3 - 0.95	7.6A	2.2J	8.4	0.1	1.1	12.9I	8.53
	0.95 - 1.3	8.5A	2.1B	10	0.14	2.2	17B	12.94
	2.3E	10	0.11	2	11.76
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.95
	0.95 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.95
	0.95 - 1.3

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	149	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension