Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1494	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	26/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7711568 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	359429  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Black Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.47
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa species, Aristida species
	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Eremophila mitchellii, Lysiphillum carronii, Bursaria incana
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam, fine sandy; Weak grade of structure, 2-5 
	mm, Platy; Rough-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.01); Abrupt change to - 
	A12	0.02 - 0.18 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy light clay; Weak grade of structure, 10-20 
	mm, Angular blocky; Rough-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, 
	, ; Field pH 5.5 (Raupach, 0.1); Abrupt change to - 
	A2j	0.18 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Fine sandy light clay (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach,
	 0.2); Clear change to - 
	B21	0.2 - 0.5 m	Very dark grey (10YR3/1-Moist); ; Sandy light medium clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1494	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.18	5.2A
	0.2 - 0.5	5.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.18
	0.2 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.18
	0.2 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1494	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension