Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	15	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	25/06/90	Elevation:	165 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7744864 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	491714  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol Thick Non-gravelly Sandy 	Principal Profile Form:	Uc5.21
	Sandy Very deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Eragrostis species, Chrysopogon fallax, Heteropogon contortus
	Mid Strata - , , . *Species includes - Jatropha gossypifolia, Petalostigma pubescens, Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Planchonia 
	careya
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Brown (10YR4/3-Moist); ; Fine sand; Massive grade of structure; Moderately moist; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Ferricrete; Field pH 5.8 (Raupach, 0.05); Many, fine
	 (1-2mm) roots; Clear, Smooth change to - 
	A12	0.08 - 0.32 m	Dark yellowish brown (10YR4/4-Moist); ; Fine sand; Massive grade of structure; Moderately 
	moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Ferricrete; Field pH 6 (Raupach, 
	0.3); Few, very fine (0-1mm) roots; Diffuse, Smooth change to - 
	B21	0.32 - 1.35 m	Strong brown (7.5YR4/6-Moist); ; Fine sand; Massive grade of structure; Moderately moist; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Ferricrete; Field pH 6.5 (Raupach, 0.7); Few, 
	very fine (0-1mm) roots; Gradual, Smooth change to - 
	B3	1.35 - 2.05 m	Strong brown (7.5YR5/8-Moist); ; Loamy fine sand; Massive grade of structure; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Ferricrete; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	15	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.6A	2.5B	1.1	0.31	0.04
	0.08 - 0.32	7.1A
	0.32 - 1.35	7.3A	3.1J	1.3	0.3	0	6.4I	0.00
	1.35 - 2.05	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.32
	0.32 - 1.35
	1.35 - 2.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.32
	0.32 - 1.35
	1.35 - 2.05

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	15	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension