Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1506	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	12/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7721181 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	369741  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Massive Black Vertosol Non-gravelly Medium fine Very 	Principal Profile Form:	Ug5.4
	fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Aristida species, Themeda 
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; 
	Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Abrupt change to - 
	A2e	0.05 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Light medium clay; Massive grade of structure; Earthy 
	fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.08); Abrupt change to - 
	B21	0.08 - 0.45 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Smooth-ped fabric; Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.6 (Raupach, 0.3); Clear change to - 
	B22	0.45 - 0.8 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, 
	coarse fragments; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; , 
	Gypseous, , ; Soil matrix is Very highly calcareous; Field pH 8.5 (Raupach, 0.6); Gradual 
	change to - 
	B23	0.8 - 1.2 m	Light brownish grey (2.5Y6/2-Moist); ; Medium clay (Light); Moderate grade of structure, 20-50 
	mm, Angular blocky; Moderate grade of structure, 5-10 mm, Polyhedral; Smooth-ped fabric; 
	Moderately moist; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly calcareous; Field pH 8 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1506	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1506	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile