Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1507	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	12/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7721386 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	367624  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroferric Brown Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn2.21
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida species, Chrysopogon fallax, Heteropogon 
	contortus	Mid Strata - Tree, 1.01-3m, Mid-dense. *Species includes - Eucalyptus melanophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (10YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Abrupt 
	change to - 
	A12	0.05 - 0.15 m	Brown (10YR5/3-Moist); ; Sandy clay loam; Massive grade of structure; Sandy (grains prominent)
	 fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear change to - 
	B21	0.15 - 0.4 m	Light olive brown (2.5Y5/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.3); Clear change to - 
	B22	0.4 - 0.75 m	Olive yellow (2.5Y6/6-Moist); Mottles, 10YR56, 2-10% , 0-5mm, Prominent; Mottles, 2-10% ; 
	Sandy light clay; Massive grade of structure; Earthy fabric; Dry; 10-20%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1507	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1507	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile