Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1517	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	13/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7717564 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	363110  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cryptogam surface
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol Thin Non-gravelly Clay-	Principal Profile Form:	Gn2.41
	loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable group
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Chrysopogon fallax, Aristida 
	species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Grevillea species
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.05 m	Brown (10YR4/3-Moist); ; Sandy clay loam; Massive grade of structure; Sandy (grains prominent)
	 fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); 
	Abrupt change to - 
	B1	0.05 - 0.2 m	Dark yellowish brown (10YR4/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.15); 
	Clear change to - 
	B2	0.2 - 0.4 m	Dark yellowish brown (10YR4/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1517	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1517	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile