Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	14/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7698820 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	365573  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Low hills
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Reticulate Eutrophic Grey Kandosol Thin Non-gravelly Loamy 	Principal Profile Form:	Dg2.81
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - Triodia mitchelii, Heteropogon contortus, Themeda
	 triandra	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Massive grade of structure; , Calcareous, , ; ,
	 Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear change to - 
	A21e	0.05 - 0.2 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; , Calcareous, , ; , Gypseous, ,
	 ; Field pH 6 (Raupach, 0.15); Clear change to - 
	A22e	0.2 - 0.45 m	Light yellowish brown (10YR6/4-Moist); ; Sandy clay loam; Massive grade of structure; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Clear change to - 
	B2	0.45 - 0.85 m	Pale brown (10YR6/3-Moist); Mottles, 10YR56, 10-20% , 5-15mm, Prominent; Mottles, 10-20% ; 
	Sandy clay loam; Massive grade of structure; Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm),
	 Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A
	0.05 - 0.2	6.1A
	0.2 - 0.45	5.6A
	0.45 - 0.85	6.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.45
	0.45 - 0.85
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.45
	0.45 - 0.85

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension