Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1526	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	14/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7692382 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	359361  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Medium Non-gravelly Sandy 	Principal Profile Form:	Gn2.12
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon triticeus, Chrysopogon fallax, 
	Heteropogon contortus	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Acacia species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus similis
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.03 m	Dark reddish brown (5YR3/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.05); Abrupt change to - 
	A12	0.03 - 0.2 m	Reddish brown (5YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Clear change 
	to - 
	B21	0.2 - 0.5 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.4); Clear change to - 
	B22	0.5 - 0.8 m	Red (2.5YR4/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.7); Clear change to -
	B23	0.8 - 0.85 m	Red (2.5YR4/8-Moist); ; Sandy light clay; Massive grade of structure; Sandy (grains prominent) 
	fabric; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.85); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1526	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	6A
	0.03 - 0.3	6.4A
	0.2 - 0.5	6.4A
	0.8 - 0.85	6.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2
	0.03 - 0.3
	0.2 - 0.5
	0.8 - 0.85
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.03 - 0.3
	0.2 - 0.5
	0.8 - 0.85

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1526	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension