Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1543	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	27/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7680549 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	388708  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Mesotrophic Brown Dermosol Medium Non-gravelly 	Principal Profile Form:	Dy2.13
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Acacia shirleyi
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Acacia argyrodendron
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Clay loam, fine sandy; Strong grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ;
	 Field pH 7 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.5 m	Dark greyish brown (2.5Y4/3-Moist); ; Light medium clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; Few (2 - 10 %), Calcareous, 
	Medium (2 -6 mm), Nodules; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 
	(Raupach, 0.3); Gradual change to - 
	B22	0.5 - 0.95 m	Dark greyish brown (2.5Y4/2-Moist); ; Light medium clay; Moderate grade of structure, 20-50 mm,
	 Subangular blocky; Weak grade of structure, Lenticular; Smooth-ped fabric; Moderately moist; 
	Very firm consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly calcareous; Field pH 8.5 (Raupach, 0.7); 
	Gradual change to - 
	B23	0.95 - 1.2 m	Dark greyish brown (2.5Y4/2-Moist); ; Light medium clay (Light); Moderate grade of structure, 20-
	50 mm, Subangular blocky; Weak grade of structure, Lenticular; Smooth-ped fabric; Moderately 
	moist; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is Slightly calcareous; 
	Field pH 9 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1543	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.5A	13B	4.9	0.67	0.69
	0.1 - 0.5	8A
	0.5 - 0.95	8.1A
	0.95 - 1.2	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.5
	0.5 - 0.95
	0.95 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.5
	0.5 - 0.95
	0.95 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1543	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension