Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1550	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	28/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   GPS	Rainfall:	No Data
	Northing/Long.:	7716102 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	331141  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Thick Non-gravelly Loamy	Principal Profile Form:	Dy2.61
	 Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - TRIODIA SPECIES ?, Chrysopogon fallax, 
	Heteropogon contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus similis, Eucalyptus shirleyi, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.04); Clear change to - 
	A12	0.08 - 0.3 m	Dark yellowish brown (10YR3/4-Moist); ; Clayey sand (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B21	0.3 - 0.55 m	Yellowish brown (10YR5/6-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; 10-20%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; 
	Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ;
	 Field pH 6 (Raupach, 0.4); Clear change to - 
	B22	0.55 - 0.8 m	Yellowish brown (10YR5/8-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; Very many (50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1550	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1550	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile