Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1565	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	29/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   GPS	Rainfall:	No Data
	Northing/Long.:	7728970 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	322690  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Thick Slightly gravelly 	Principal Profile Form:	Dr3.11
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Chrysopogon fallax, Aristida species, 
	Heteropogon contortus	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Acacia species, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/3-Moist); ; Sandy loam; Massive grade of structure; Dry; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Clayey sand (Heavy); Massive grade of structure; Dry; Very weak 
	consistence; 50-90%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Abrupt change to - 
	B2	0.3 - 0.8 m	Red (10R4/8-Moist); Mottles, 7.5YR56, 10-20% , Faint; Mottles, 10-20% ; Medium clay; Moderate 
	grade of structure, 20-50 mm, Angular blocky; Moderate grade of structure, Lenticular; 
	Moderately moist; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1565	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.5A	2.2B	1.4	0.33	0.03
	0.1 - 0.3	5.5A
	0.3 - 0.8	5.7A	0.88B	14	0.28	0.46
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1565	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension