Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	29/10/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   GPS	Rainfall:	No Data
	Northing/Long.:	7725958 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	329188  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Yellow Chromosol Thick Non-gravelly Sandy	Principal Profile Form:	Dy3.52
	 Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Chrysopogon fallax, Aristida 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Massive grade of structure; Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); 
	A12	0.05 - 0.12 m	Brown (10YR5/3-Moist); ; Clayey sand; Massive grade of structure; Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.1); 
	A13	0.12 - 0.32 m	Yellowish brown (10YR5/4-Moist); ; Clayey sand; Massive grade of structure; Dry; Firm 
	consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.2); 
	B2	0.32 - 0.45 m	Brownish yellow (10YR6/8-Moist); ; Sandy light clay; Massive grade of structure; Dry; Strong 
	consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Few (2 - 10 
	%), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.05 - 0.12	6.2A	1.8B	0.54	0.17	0.02
	0.12 - 0.32	6.2A
	0.32 - 0.45	6A	2.2B	1.7	0.19	0.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.05 - 0.12
	0.12 - 0.32
	0.32 - 0.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.05 - 0.12
	0.12 - 0.32
	0.32 - 0.45

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension