Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1596	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7958   GPS	Rainfall:	No Data
	Northing/Long.:	7811458 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	330293  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Medium Gravelly Clay-loamy 	Principal Profile Form:	Gn3.22
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	Euchrozem
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Themeda triandra, 
	Chrysopogon fallax	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	10-20%, stony, 200-600mm, rounded, Basalt
	Profile Morphology
	A11	0 - 0.07 m	Dark reddish brown (5YR3/2-Moist); ; Clay loam; Weak grade of structure; Earthy fabric; Dry; Very
	 firm consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; ,
	 Gypseous, , ; Field pH 6.5 (Raupach, 0.03); 
	A12	0.07 - 0.25 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Polyhedral; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Strong 
	consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.2); 
	B2	0.25 - 0.45 m	Dark reddish brown (5YR3/4-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1596	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1596	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile