Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	16	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	25/06/90	Elevation:	170 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7745472 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	491506  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Level
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Very thick Non-gravelly 	Principal Profile Form:	Dy4.82
	Sandy Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	No suitable group
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Eragrostis species, Bothriochloa pertusa, Perotis rara
	Mid Strata - , , . *Species includes - Eucalyptus platyphylla, Eucalyptus brownii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Brown (10YR4/3-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) fabric; Dry;
	 Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Few, very
	 fine (0-1mm) roots; Clear, Smooth change to - 
	A12	0.12 - 0.48 m	Yellowish brown (10YR5/6-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.3); Few, very fine (0-1mm) roots; Diffuse, Smooth change to - 
	A21	0.48 - 1 m	Yellowish brown (10YR5/6-Moist); ; Clayey coarse sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; Very weak consistence; 0-2%, medium gravelly, 6-
	20mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	(Raupach, 0.6); Field pH 6.8 (Raupach, 1); Clear, Smooth change to - 
	A22e	1 - 1.22 m	Yellowish brown (10YR5/6-Moist); ; Clayey coarse sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; Very weak consistence; 2-10%, medium gravelly, 6-
	20mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth 
	change to - 
	B21	1.22 - 1.6 m	Yellowish brown (10YR5/6-Moist); ; Coarse sandy clay loam; Weak grade of structure, 20-50 
	mm, Prismatic; Smooth-ped fabric; Moderately moist; Firm consistence; 10-20%, medium 
	gravelly, 6-20mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 1.3); Clear, Smooth change to - 
	B22	1.6 - 1.9 m	Yellowish brown (10YR5/6-Moist); Mottles, 2.5Y78, 0-2% , 0-5mm, Distinct; Mottles, 0-2% ; 
	Coarse sandy clay loam; Weak grade of structure, 20-50 mm, Prismatic; Smooth-ped fabric; 
	Moist; Firm consistence; 20-50%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; 
	, Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	16	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	7.7A	3.1B	0.9	0.32	0.04
	0.12 - 0.48	8A
	0.48 - 1	8.2A	1.9B	0.75	0.11	0.05
	1 - 1.22	8A
	1.22 - 1.6	8.3A	5.7J	2	0.5	0	10.5I	0.00
	1.6 - 1.9	8.4A	5.7B	2.1	0.38	0.1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.48
	0.48 - 1
	1 - 1.22
	1.22 - 1.6
	1.6 - 1.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.48
	0.48 - 1
	1 - 1.22
	1.22 - 1.6
	1.6 - 1.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	16	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension