Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1602	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	01/02/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8059   GPS	Rainfall:	No Data
	Northing/Long.:	7887566 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	368771  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Thin Very gravelly Loamy 	Principal Profile Form:	Db1.52
	Clay-loamy Shallow
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra, Heteropogon contortus, 
	Bothriochloa species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, angular tabular, 
	Profile Morphology
	A1	0 - 0.07 m	Dark brown (7.5YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Moist; Very
	 weak consistence; 50-90%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	B2	0.07 - 0.28 m	Strong brown (7.5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; 50-90%, coarse gravelly, 20-60mm, angular, 
	Substrate material, coarse fragments; , Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) 
	roots; Clear change to - 
	C	0.28 - 0.48 m	Yellowish brown (10YR5/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Weak consistence; 50-90%, 
	coarse gravelly, 20-60mm, angular, Substrate material, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1602	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	7.5A	0.06A	3.6B	0.05
	0.07 - 0.28	4.6C	0.05A
	7.1A
	0.28 - 0.48	7.1A	0.05A	1.1B	6.8	0.14	0.33
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	1.8A	0.043A	0.08A	2.7A	35A	38	15	12
	0.07 - 0.28
	0.28 - 0.48	0.026A	3.04A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.28
	0.28 - 0.48

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1602	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method