Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1609	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	02/11/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7848311 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	301179  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	10 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Very gravelly Loamy 	Principal Profile Form:	Gn3.12
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra, Heteropogon contortus, 
	Heteropogon triticeus	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, angular, Quartzite
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Sandy loam; Moderate grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Dry; Firm consistence; 20-50%, coarse gravelly, 20-60mm, angular, 
	Quartzite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear 
	change to - 
	B21	0.1 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; 50-90%, coarse gravelly, 20-
	60mm, angular, Quartzite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.2); Gradual change to - 
	B22	0.3 - 0.7 m	Strong brown (7.5YR4/6-Moist); Mottles, 10R46, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ; 
	Light clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Dry; 
	Firm consistence; 50-90%, coarse gravelly, 20-60mm, angular, Quartzite, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1609	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1609	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile