Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1630	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	21/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7955   GPS	Rainfall:	No Data
	Northing/Long.:	7638126 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	344690  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Silpanic Bleached-Leptic Tenosol Very thick Non-	Principal Profile Form:	Uc2
	gravelly Sandy Sandy Deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - Triodia mitchelii
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Melaleuca tamariscina, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy coarse sand; Massive grade of structure; Dry; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); 
	A12	0.08 - 0.5 m	Brown (10YR4/3-Moist); ; Coarse sandy loam; Massive grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.3); 
	A2e	0.5 - 0.7 m	Brown (10YR5/3-Moist); ; Clayey sand; Single grain grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.7); 
	0.7 - 0.8 m	White (10YR8/1-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Densipan, Weakly cemented, 
	Continuous, Massive; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1630	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1630	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile