Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1662	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	29/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7958   GPS	Rainfall:	No Data
	Northing/Long.:	7840422 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	314042  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	No Data
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Self-Mulching Black Vertosol Non-gravelly 	Principal Profile Form:	Ug5.11
	Fine Medium fine Shallow 
	ASC Confidence:	Great Soil Group:	Black earth
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa species, Ophiurous exaltatus, Cyperus 
	species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus 
	Surface Coarse Fragments:	0-2%, cobbly, 60-200mm, subrounded, 
	Profile Morphology
	A11	0 - 0.03 m	Dark brown (10YR3/3-Moist); ; Light medium clay; Strong grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Dry; Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), 
	Nodules; , Gypseous, , ; Field pH 7 (Raupach, 0.02); Clear change to - 
	B21	0.03 - 0.4 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Prismatic; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH
	 7 (Raupach, 0.2); Gradual change to - 
	BD	0.4 - 0.55 m	; Weak grade of structure, 20-50 mm, Subangular blocky; Dry; Very firm consistence; 10-20%, 
	medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; Few cutans, <10% 
	of ped faces or walls coated, distinct; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 
	0.5); Gradual change to - 
	D	0.55 - 0.7 m	; Dry; Firm consistence; 10-20%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1662	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1662	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile