Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1668	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	04/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8159   GPS	Rainfall:	No Data
	Northing/Long.:	7859655 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	396347  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust, Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Crusty Grey Vertosol Gravelly Medium fine Very	Principal Profile Form:	Uf6
	 fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - , , . *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, rounded, 
	Profile Morphology
	A11	0 - 0.02 m	Brown (10YR4/3-Moist); ; Light clay; Moderate grade of structure, <2 mm, Platy; Smooth-ped 
	fabric; Dry; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; Very few 
	(0 - 2 %), Manganiferous, , Nodules; Common (10 - 20 %), Calcareous, Fine (0 - 2 mm), Nodules;
	 , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9.5 (Raupach, 0.02); 
	A12	0.02 - 0.35 m	Brown (10YR4/3-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Angular blocky; 
	Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Dry; 2-10%, fine gravelly, 
	2-6mm, rounded, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Manganiferous, , 
	Nodules; Common (10 - 20 %), Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Soil matrix
	 is Highly calcareous; Field pH 9.5 (Raupach, 0.25); 
	B21	0.35 - 0.8 m	Dark grey (10YR4/1-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, Lenticular; 
	Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Moderately moist; 2-10%, 
	fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; Very many (50 - 100 %), , , ; 
	, Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	B22	0.8 - 1.2 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, 
	Lenticular; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Moderately 
	moist; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; Very many 
	(50 - 100 %), , , ; , Calcareous, , ; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9.5 
	(Raupach, 1); 
	B23	1.2 - 1.4 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR58, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ; 
	Medium clay; Strong grade of structure, 5-10 mm, Angular blocky; Strong grade of structure, 2-5 
	mm, Angular blocky; Smooth-ped fabric; Moderately moist; 2-10%, fine gravelly, 2-6mm, 
	rounded, dispersed, Quartz, coarse fragments; Very many (50 - 100 %), , , ; , Calcareous, , ; , 
	Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9.5 (Raupach, 1.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1668	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1668	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile