Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1675	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	05/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8159   GPS	Rainfall:	No Data
	Northing/Long.:	7866392 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	403832  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Chromosol Medium Gravelly Clay-	Principal Profile Form:	Dy3.31
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Soloth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Themeda triandra
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, rounded, Unconsolidated material (unidentified)
	Profile Morphology
	A11	0 - 0.1 m	Brown (10YR5/3-Moist); ; Sandy clay loam; Massive grade of structure; , Calcareous, , ; , 
	Gypseous, , ; 
	A2j	0.1 - 0.25 m	Yellowish brown (10YR5/4-Moist); ; Sandy clay loam; Massive grade of structure; , Calcareous, ,
	 ; , Gypseous, , ; 
	B21	0.25 - 0.5 m	Strong brown (7.5YR5/6-Moist); Mottles, 2.5YR36, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ; 
	Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 2-10%, medium 
	gravelly, 6-20mm, rounded tabular, dispersed, Unconsolidated material (unidentified), coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; 
	B22	0.5 - 0.8 m	Grey (10YR6/1-Moist); Mottles, 2.5YR36, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ; Medium 
	heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 10-20%, coarse gravelly, 20-
	60mm, rounded tabular, dispersed, Unconsolidated material (unidentified), coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1675	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1675	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile