Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	21/09/90	Elevation:	650 metres
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7951563 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	274784  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	150 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Brown Ferrosol Thin Non-gravelly Clay-loamy 	Principal Profile Form:	Gn3.25
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Xanthozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Themeda triandra, 
	Dichanthium species	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus brownii
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus platyphylla, Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1c	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam (Heavy); Strong grade of structure, 5-10 
	mm, Cast; Strong grade of structure, <2 mm, Granular; Earthy fabric; Many (>5 per 100mm2) Fine
	 (1-2mm) macropores, Dry; Very weak consistence; Common (10 - 20 %), Manganiferous, Fine (0
	 - 2 mm), Concretions; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Common, 
	fine (1-2mm) roots; Clear, Smooth change to - 
	A3c	0.05 - 0.2 m	Dark yellowish brown (10YR3/4-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Granular; 
	Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; 
	Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Concretions; , Calcareous, , ; , Gypseous,
	 , ; Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	B21c	0.2 - 0.55 m	Dark yellowish brown (10YR4/6-Moist); ; Light medium clay; Strong grade of structure, 2-5 mm, 
	Polyhedral; Smooth-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately 
	moist; Weak consistence; Many (20 - 50 %), Ferromanganiferous, Medium (2 -6 mm), 
	Concretions; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.55); Common, fine (1-2mm)
	 roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.7A	13B	6.1	1.4	0.06
	0.2 - 0.55	7A	4B	4.4	0.32	0.14	12.4I	1.13
	6.4J	4.9	0.4	0.1	0.81
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.2 - 0.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.2 - 0.55

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	169	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension